IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "RevitIdentifiers [VersionGUID: 2996e929-e8fa-4238-915a-9c109cefc0de, NumberOfSaves: 1]"
Description: "CoordinateReference [CoordinateBase: Interner Ursprung, ProjectSite: Intern]"
Description: "ExchangeRequirement [Architecture]"
File name: "2018_01"
Time stamp: "2024-03-06T17:56:29+01:00"
Preprocessor: "ODA SDAI 24.6"
Originating system: "Autodesk Revit 24.2.0.63 (DEU) - IFC 24.2.0.63"
Application: "Autodesk Revit 2024 (DEU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (DEU)"

People and organizations
  Person "lucas.marques7KKVS" of Organization (no name given)
  Owner history of Person "lucas.marques7KKVS" of Organization (no name given) | application "Autodesk Revit 2024 (DEU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (DEU)" | change NOCHANGE | created 1709743277 (2024-03-06T16:41:17Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  CURRENCY: €
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  AREADENSITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "2018_01" | phase "Projekt Status"
  IFCSITE "Default" | latitude 48° 8′ 15.359802″ | longitude 11° 34′ 47.783432″ | elevation above sea level 0.
    contains 1 element
      1 x IFCWINDOW | type IFCWINDOWTYPE "Groeninger Window Drives:Window actuator DK-100 (Art. No. G1001000)" | object type "Groeninger Window Drives:Window actuator DK-100 (Art. No. G1001000)" | WINDOW | names: "Groeninger Window Drives:Window actuator DK-100 (Art. No. G1001000):2514764" | material: constituents ("<Unnamed>": "<Unnamed>", "Modelltext blau": "Modelltext blau") | property sets: PSET_DK 100_Description, PSET_DK 100_Electrical supply, PSET_DK 100_Features, PSET_DK 100_Fitting requirements, PSET_DK 100_Manufacturer, PSET_DK 100_Profile Requirements

Types
  IFCWINDOWTYPE "Groeninger Window Drives:Window actuator DK-100 (Art. No. G1001000)" | WINDOW | 1 occurrence | material: constituents ("<Unnamed>": "<Unnamed>", "Modelltext blau": "Modelltext blau") | property sets: Groeninger Window Drives:Window actuator DK-100 (Art. No. G1001000):2514764

Property sets
  PSET_DK 100_Description | properties | on 1 object (1 IFCWINDOW)
    Description = "Window drive for automated tilt-opening and tilt-closing including locking and unlocking, with full retention of manual operation in any window position and completely concealed frame mounting" (IFCTEXT)
  PSET_DK 100_Electrical supply | properties | on 1 object (1 IFCWINDOW)
    Duty cycle (DIN EN 60034-1) = "S3 25%; S2 2min" (IFCTEXT)
    Rated current consumption = "0.75 A" (IFCTEXT)
    Risidual ripple = "max. 2Vp-p" (IFCTEXT)
    Supply voltage by external power supply = "24V DC" (IFCTEXT)
  PSET_DK 100_Features | properties | on 1 object (1 IFCWINDOW)
    Building Management System / Smart Home = "Integration into the building management system through potential-free normally open contact (digital IO)" (IFCTEXT)
    Control = "Pushbuttons, switches, dead man's buttons" (IFCTEXT)
    Detection of window position = "Detection of the window position integrated in the drive during automatic and manual operation" (IFCTEXT)
    End positions = "Automated referencing of end positions" (IFCTEXT)
    Hinge side = "Hinge side right and left possible" (IFCTEXT)
    Installation position = "Completely concealed drive milled into the profile, invisible in closed position" (IFCTEXT)
    Lifetime = "Tested with 20,000 switching cycles (double stroke incl. locking)" (IFCTEXT)
    Manual operation = "Manual operation of all window positions (tilt position, turning position, closed position) by window handle possible from any position (window handle permanently mounted)" (IFCTEXT)
    Opening / Closing Time = "approx. 28s in normal mode and approx. 35s in slow mode" (IFCTEXT)
    Opening and closing force = "800N via the locking bar" (IFCTEXT)
    Opening width = "Tilt opening width between 100 mm and 130 mm depending on the fitting used" (IFCTEXT)
    Reduced speed = "Slow mode adjustable via DIP switch to realize quiet running noise" (IFCTEXT)
    Window type = "Suitable for rectangular tilt-and-turn windows made of wood, plastic or aluminium" (IFCTEXT)
  PSET_DK 100_Fitting requirements | properties | on 1 object (1 IFCWINDOW)
    Accessories = "No additional components required, such as brackets for drive attachment or elements for transmitting the drive force, are required" (IFCTEXT)
    Possible fittings = "Winkhaus activPilot Ergo, Maco Multi Comfort Fitting" (IFCTEXT)
    max. sash weight = "60 kg" (IFCTEXT)
  PSET_DK 100_Manufacturer | properties | on 1 object (1 IFCWINDOW)
    City = "Aichtal" (IFCTEXT)
    Company = "Groeninger Antriebstechnik GmbH & Co. KG" (IFCTEXT)
    Country = "Germany" (IFCTEXT)
    Email = "info@fenster-antrieb.de" (IFCTEXT)
    Street = "Alte Str. 9" (IFCTEXT)
    Telephone = "+49 7127 9606380" (IFCTEXT)
    Website = "www.fenster-antrieb.de" (IFCTEXT)
    Zip code = "72631" (IFCTEXT)
  PSET_DK 100_Profile Requirements | properties | on 1 object (1 IFCWINDOW)
    Center sealing = "Center sealing systems required" (IFCTEXT)
    Fastening = "Sufficient material available for screw fastening" (IFCTEXT)
    Groove position = "13mm" (IFCTEXT)
    Rebate space = "12-14mm" (IFCTEXT)
    Space = "Installation space Available in the lower frame piece" (IFCTEXT)
  PSET_DK 100_Scope of delivery | properties | on 1 object (1 IFCWINDOW)
    Scope of delivery = "DriveConnecting cable 3m PVCFastening screws for plastic windowsCover connection area incl. strain relief and screwsMagnet for position detectionSticker "Power-operated window"" (IFCTEXT)
  Groeninger Window Drives:Window actuator DK-100 (Art. No. G1001000):2514764 | predefined | on 1 type object